diff -P -u -x '*~' -x '\.*' -r SF35-Makerbot-baseline/alterations/end.gcode SF35-Thingomatic-baseline/alterations/end.gcode
--- SF35-Makerbot-baseline/alterations/end.gcode	2011-02-03 14:30:23.000000000 +0100
+++ SF35-Thingomatic-baseline/alterations/end.gcode	2011-02-04 15:04:54.000000000 +0100
@@ -1,2 +1,24 @@
 (**** Beginning of end.gcode ****)
+(This file is for a MakerBot Thing-O-Matic)
+(*** begin settings ****)
+M109 S95 T0 (set heated-build-platform temperature)
+(**** end settings ****)
+(**** begin move to cooling position ****)
+G1 X0.0 F3300.0       (move to cooling position)
+G1 X0.0 Y55.0 F3300.0 (move to cooling position)
+(**** end move to cooling position ****)
+(**** begin filament reversal ****)
+M102 (Extruder on, reverse)
+G04 P2000 (Wait t/1000 seconds)
+M103 (Extruder off)
+(**** end filament reversal ****)
+M18 (Turn off steppers)
+(**** begin eject ****)
+M6 T0 (wait for toolhead parts (nozzle, HBP, etc) to reach temperature)
+M01 (Remove the object then click yes.)
+(**** end eject ****)
+(**** begin cool for safety ****)
+M104 S0 T0 (set extruder temperature)
+M109 S0 T0 (set heated-build-platform temperature)
+(**** end cool for safety ****)
 (**** end of end.gcode ****)
diff -P -u -x '*~' -x '\.*' -r SF35-Makerbot-baseline/alterations/start.gcode SF35-Thingomatic-baseline/alterations/start.gcode
--- SF35-Makerbot-baseline/alterations/start.gcode	2011-02-04 15:17:10.000000000 +0100
+++ SF35-Thingomatic-baseline/alterations/start.gcode	2011-02-04 15:04:54.000000000 +0100
@@ -1,4 +1,5 @@
 (**** beginning of start.gcode ****)
+(This file is for a MakerBot Thing-O-Matic)
 (**** begin initialization commands ****)
 G21 (set units to mm)
 G90 (set positioning to absolute)
@@ -8,5 +9,16 @@
 M109 S125 T0 (set heated-build-platform temperature)
 (**** end initialization commands ****)
 (**** begin homing ****)
+G162 Z F500 (home Z axis maximum)
+G161 X Y F2500 (home XY axes minimum)
+G92 Z80 ( ---=== Set Z axis maximum ===--- )
+G92 X-57.5 Y-57 (set zero for X and Y)
 (**** end homing ****)
+(**** begin pre-wipe commands ****)
+G1 X52 Y-57.0 Z10 F3300.0 (move to waiting position)
+M6 T0 (wait for toolhead parts, nozzle, HBP, etc., to reach temperature)
+M101 (Extruder on, forward)
+G04 P5000 (Wait t/1000 seconds)
+M103 (Extruder off)
+(**** end pre-wipe commands ****)
 (**** end of start.gcode ****)
