speed.csv:Feed Rate (mm/s):=28.0
carve.csv:Layer Thickness (mm):=0.39
fill.csv:Infill Perimeter Overlap (ratio):=0.4
fill.csv:Infill Solidity (ratio):=0.4
fill.csv:Extra Shells on Alternating Solid Layer (layers):=1
fill.csv:Extra Shells on Base (layers):=1
inset.csv:Overlap Removal Width over Perimeter Width (ratio):=0.7
