diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/alterations/end.gcode SF35-Thingomatic-HBP-Stepstruder/alterations/end.gcode
--- SF35-Thingomatic-HBP/alterations/end.gcode	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/alterations/end.gcode	2011-02-04 17:50:42.000000000 +0100
@@ -8,6 +8,7 @@
 G1 X0.0 Y55.0 F3300.0 (move to cooling position)
 (**** end move to cooling position ****)
 (**** begin filament reversal ****)
+M108 R1.98 (set extruder speed)
 M102 (Extruder on, reverse)
 G04 P2000 (Wait t/1000 seconds)
 M103 (Extruder off)
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/alterations/replace.csv SF35-Thingomatic-HBP-Stepstruder/alterations/replace.csv
--- SF35-Thingomatic-HBP/alterations/replace.csv	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/alterations/replace.csv	2011-02-04 17:50:42.000000000 +0100
@@ -1 +1,2 @@
 M113	;M113
+M108 S	M108 R
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/alterations/start.gcode SF35-Thingomatic-HBP-Stepstruder/alterations/start.gcode
--- SF35-Thingomatic-HBP/alterations/start.gcode	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/alterations/start.gcode	2011-02-04 17:50:42.000000000 +0100
@@ -3,7 +3,7 @@
 (**** begin initialization commands ****)
 G21 (set units to mm)
 G90 (set positioning to absolute)
-M108 S255 (set extruder speed to maximum)
+M108 R1.98 (set extruder speed)
 M103 (Make sure extruder is off)
 M104 S225 T0 (set extruder temperature)
 M109 S125 T0 (set heated-build-platform temperature)
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/alterations/start.gcode.orig SF35-Thingomatic-HBP-Stepstruder/alterations/start.gcode.orig
--- SF35-Thingomatic-HBP/alterations/start.gcode.orig	1970-01-01 01:00:00.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/alterations/start.gcode.orig	2011-02-04 17:50:42.000000000 +0100
@@ -0,0 +1,24 @@
+(**** beginning of start.gcode ****)
+(This file is for a MakerBot Thing-O-Matic)
+(**** begin initialization commands ****)
+G21 (set units to mm)
+G90 (set positioning to absolute)
+M108 S255 (set extruder speed to maximum)
+M103 (Make sure extruder is off)
+M104 S225 T0 (set extruder temperature)
+M109 S125 T0 (set heated-build-platform temperature)
+(**** end initialization commands ****)
+(**** begin homing ****)
+G162 Z F500 (home Z axis maximum)
+G161 X Y F2500 (home XY axes minimum)
+G92 Z80 ( ---=== Set Z axis maximum ===--- )
+G92 X-57.5 Y-57 (set zero for X and Y)
+(**** end homing ****)
+(**** begin pre-wipe commands ****)
+G1 X52 Y-57.0 Z10 F3300.0 (move to waiting position)
+M6 T0 (wait for toolhead parts, nozzle, HBP, etc., to reach temperature)
+M101 (Extruder on, forward)
+G04 P5000 (Wait t/1000 seconds)
+M103 (Extruder off)
+(**** end pre-wipe commands ****)
+(**** end of start.gcode ****)
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/profiles/extrusion/ABS/carve.csv SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/carve.csv
--- SF35-Thingomatic-HBP/profiles/extrusion/ABS/carve.csv	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/carve.csv	2011-02-04 17:50:42.000000000 +0100
@@ -12,5 +12,5 @@
 Layers To (index):	912345678
 Correct Mesh	True
 Unproven Mesh	False
-Perimeter Width over Thickness (ratio):	1.45
+Perimeter Width over Thickness (ratio):	1.25
 SVG Viewer:	webbrowser
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/profiles/extrusion/ABS/cool.csv SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/cool.csv
--- SF35-Thingomatic-HBP/profiles/extrusion/ABS/cool.csv	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/cool.csv	2011-02-04 17:51:13.000000000 +0100
@@ -2,7 +2,7 @@
 Name                          	Value
 WindowPosition	700+0
 Open File for Cool	
-Activate Cool	False
+Activate Cool	True
 Orbit	False
 Slow Down	True
 Maximum Cool (Celcius):	0.0
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/profiles/extrusion/ABS/fill.csv SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/fill.csv
--- SF35-Thingomatic-HBP/profiles/extrusion/ABS/fill.csv	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/fill.csv	2011-02-04 17:50:42.000000000 +0100
@@ -23,7 +23,7 @@
 Line	False
 Infill Perimeter Overlap (ratio):	0.35
 Infill Solidity (ratio):	0.25
-Infill Width over Thickness (ratio):	1.5
+Infill Width over Thickness (ratio):	1.25
 Solid Surface Thickness (layers):	2
 Infill > Loops > Perimeter	False
 Infill > Perimeter > Loops	False
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/profiles/extrusion/ABS/reversal.csv SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/reversal.csv
--- SF35-Thingomatic-HBP/profiles/extrusion/ABS/reversal.csv	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/reversal.csv	2011-02-04 17:50:42.000000000 +0100
@@ -2,7 +2,7 @@
 Name                          	Value
 WindowPosition	700+0
 Open File for Reversal	
-Activate Reversal	False
+Activate Reversal	True
 Reversal speed (RPM):	35.0
 Reversal time (milliseconds):	70.0
 Push-back time (milliseconds):	73.0
diff -P -u -x '*~' -x '\.*' -r SF35-Thingomatic-HBP/profiles/extrusion/ABS/speed.csv SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/speed.csv
--- SF35-Thingomatic-HBP/profiles/extrusion/ABS/speed.csv	2011-02-04 17:50:42.000000000 +0100
+++ SF35-Thingomatic-HBP-Stepstruder/profiles/extrusion/ABS/speed.csv	2011-02-04 17:50:42.000000000 +0100
@@ -9,8 +9,8 @@
 Duty Cyle at Beginning (portion):	1.0
 Duty Cyle at Ending (portion):	0.0
 Feed Rate (mm/s):	32.0
-Flow Rate Setting (float):	255.0
+Flow Rate Setting (float):	1.98
 Orbital Feed Rate over Operating Feed Rate (ratio):	0.5
 Perimeter Feed Rate over Operating Feed Rate (ratio):	1.0
 Perimeter Flow Rate over Operating Flow Rate (ratio):	1.0
-Travel Feed Rate (mm/s):	32.0
+Travel Feed Rate (mm/s):	40.0
