(**** Beginning of end.txt ****)
M102 (Extruder on, reverse)
G04 P2000 (Wait t/1000 seconds)
M103 (Extruder off)
M109 S100 T0 (set heated-build-platform temperature)
G1 X0.0 Y65.0 F3300.0 (move to ejection position)
G04 P90000 (wait t/1000 seconds)
M106 (conveyor on)
G04 P2000 (wait t/1000 seconds)
M104 S220 T0 (set extruder temperature)
M109 S118 T0 (set heated-build-platform temperature)
G04 P10000 (wait t/1000 seconds)
M107 (conveyor off)
(**** start wipe ****)
G1 X47 Y-57 Z10 F3300.0
G1 X57 Y-57 Z10 F3300.0
G1 X57 Y-35 Z10 F3300.0
(**** end wipe *****)
M104 S0 T0 (set extruder temperature)
M109 S0 T0 (set heated-build-platform temperature)
(**** end of end.txt ****)
