(**** beginning of start.txt ****)
(**** begin initilization commands ****)
G21 (set units to mm)
G90 (set positioning to absolute)
G92 X0 Y0 Z0 (set origin to current position)
M108 S255 (set extruder speed to maximum)
M104 S220 T0 (set extruder temperature)
M109 S110 T0 (set heated-build-platform temperature)
(**** end initilization commands ****)
(**** begin homing ****)
G162 Z F500 (home Z axis maximum)
G161 Y F2500 (home Y axes minimum)
G162 X F2500 (home X axes maximum)
G92 X57.5 Y-57 Z114.5 (set zero)
(**** end homing ****)
(**** begin stuff commands ****)
G1 X57 Y-57 Z10 F3300.0 (move to waiting position)
G04 P30000 (Wait t/1000 seconds)
M6 T0 (wait for tool to heat up)
M101 (Extruder on, forward)
G04 P2000 (Wait t/1000 seconds)
M103 (Extruder off)
(**** end stuff commands ****)
(**** start wipe ****)
G1 X57 Y-57 Z10 F3300.0
G1 X57 Y-30 Z10 F3300.0
(**** end wipe *****)
M101
(**** end of start.txt ****)

