# Python: module skeinforge_tools.import_plugins.svg

skeinforge_tools.import_plugins.svg ($Date: 2008/21/04 $) | index /home/enrique/Desktop/backup/babbleold/script/reprap/pyRepRap/skeinforge_tools/import_plugins/svg.py

`The svg.py script is an import translator plugin to get a carving from an svg file.
An import plugin is a script in the import_plugins folder which has the function getCarving. It is meant to be run from the
interpret tool. To ensure that the plugin works on platforms which do not handle file capitalization properly, give the plugin
a lower case name.
The getCarving function takes the file name of an svg file and returns the carving.
This example gets a carving for the svg file Screw Holder Bottom.svg. This example is run in a terminal in the folder which
contains Screw Holder Bottom.svg and svg.py.
> python
Python 2.5.1 (r251:54863, Sep 22 2007, 01:43:31)
[GCC 4.2.1 (SUSE Linux)] on linux2
Type "help", "copyright", "credits" or "license" for more information.
>>> import svg
>>> svg.getCarving()
0.20000000298, 999999999.0, -999999999.0, [8.72782748851e-17, None
..
many more lines of the carving
..`

Modules

``

__init__ | skeinforge_tools.skeinforge_utilities.euclidean | skeinforge_tools.skeinforge_utilities.gcodec |

Classes

``

SVGCarving

class SVGCarving
`` | `An svg carving.`

Methods defined here:

__init__(self)
  `Add empty lists.`

__repr__(self)
  `Get the string representation of this carving.`

getCarveCornerMaximum(self)
  `Get the corner maximum of the vertices.`

getCarveCornerMinimum(self)
  `Get the corner minimum of the vertices.`

getCarveLayerThickness(self)
  `Get the layer thickness.`

getCarveRotatedBoundaryLayers(self)
  `Get the rotated boundary layers.`

parseInitialization(self)
  `Parse gcode initialization and store the parameters.`

parseLine(self, lineIndex)
  `Parse a gcode line and add it to the inset skein.`

parseSVG(self, svgText)
  `Parse SVG text and store the layers.`

setCarveBridgeLayerThickness(self, bridgeLayerThickness)
  `Set the bridge layer thickness. If the infill is not in the direction of the bridge, the bridge layer thickness should be given as None or not set at all.`

setCarveImportRadius(self, importRadius)
  `Set the import radius.`

setCarveIsCorrectMesh(self, isCorrectMesh)
  `Set the is correct mesh flag.`

setCarveLayerThickness(self, layerThickness)
  `Set the layer thickness.`

Functions

``

addPathData(line, loops)
  `Add the data from the path line.`

addTextData(line, rotatedBoundaryLayers)
  `Add the data from the text line.`

getCarving(fileName='')
  `Get the triangle mesh for the gts file.`

getValueInQuotes(name, text, value)
  `Get value in quotes after the name.`

Data
`` |  | __author__ = 'Enrique Perez (perez_enrique@yahoo.com)' __credits__ = 'Nophead <http://hydraraptor.blogspot.com/>\nArt of Illusion <http://www.artofillusion.org/>' __date__ = '$Date: 2008/21/04 $' __license__ = 'GPL 3.0' absolute_import = _Feature((2, 5, 0, 'alpha', 1), (2, 7, 0, 'alpha', 0), 16384)

Author
`` |  | Enrique Perez (perez_enrique@yahoo.com)

Credits
`` |  | Nophead <http://hydraraptor.blogspot.com/> Art of Illusion <http://www.artofillusion.org/>